Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## S

S_OK - Static variable in class android.device.SEManager
  command execute Success
scancode - Variable in class android.device.KeyMapManager.KeyEntry
  Describes the Button event scan code`android.view.KeyEvent#getScanCode()`
ScanManager - Class in android.device
  The ScanManager class provides developers access to barcode reader related in the device To decode bar codes with this class, use the following steps: Obtain an instance of BarCodeReader with ScanManager scan = new ScanManager().
ScanManager() - Constructor for class android.device.ScanManager
SEManager - Class in android.device
  The SEManager class is used to initialize and control the security processor hardware To control the security processor hardware with this class, use the following steps: You can obtain an instance of this class by calling.
SEManager() - Constructor for class android.device.SEManager
SEManager.OperationPedInputListener - Interface in android.device
  The application has to implement the appropriate listener
SEManager.PedInputListener - Interface in android.device
SEND_GOOD_READ_BEEP_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
  To set Scanner success beep or vibrate when SendBroadcast SendBroadcast Values: `WEDGE_INTENT_ACTION_NAME` `WEDGE_INTENT_DATA_STRING_TAG`
SEND_GOOD_READ_VIBRATE_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
SEND_LABEL_PREFIX_SUFFIX - Static variable in class android.device.scanner.configuration.PropertyID
setAPN(String, String, String, int, String, String, String, String, String, String, String, int, int, String, String, int, String, boolean) - Method in class android.device.DeviceManager
  Sets the APN (access point name) configurations for mobile data network
setCurrentTime(long) - Method in class android.device.DeviceManager
  Sets the current wall time, in milliseconds.
setETU(int) - Method in class android.device.IccManager
  Set the ETU.
setGrayLevel(int) - Method in class android.device.PrinterManager
  Set print gray level
setParameterInts(int[], int[]) - Method in class android.device.ScanManager
  Sets one or more label programming parameters of type Int
setParameterString(int[], String[]) - Method in class android.device.ScanManager
  Set the scanner parameter of type String at the specified indexes.
setSpeedLevel(int) - Method in class android.device.PrinterManager
  Set print speed level
setSuspendTimeout(int, byte[], byte[]) - Method in class android.device.SEManager
  This function allows to set the security processor timeout before automatic suspension.
setTriggerMode(Triggering) - Method in class android.device.ScanManager
  This method set specifies which mode to control decode.
setupPage(int, int) - Method in class android.device.PrinterManager
  Set the page size.
sle4428_password(int, byte[]) - Method in class android.device.IccManager
  Submit the transfer data, enter the personalization mode
sle4428_readMemory(int, int) - Method in class android.device.IccManager
  Read the data stored in main memory for SLE4428
sle4428_reset(byte[]) - Method in class android.device.IccManager
  reset the SLE4428
sle4428_writeMemory(int, byte[], int) - Method in class android.device.IccManager
  Write data to the main storage area SLE4428
sle4436_authenticate(int, byte[], byte[]) - Method in class android.device.IccManager
  Get the Card verification certificate
sle4436_decValue(int) - Method in class android.device.IccManager
  Reduction balance
sle4436_readBit(byte[]) - Method in class android.device.IccManager
  Read values from the Card bit
sle4436_readMemory(int, int) - Method in class android.device.IccManager
  Read the data stored in main memory for SLE4436
sle4436_regIncrease(int) - Method in class android.device.IccManager
  Move the register
sle4436_reloadByte() - Method in class android.device.IccManager
  Reload Byte
sle4436_reset(byte[]) - Method in class android.device.IccManager
  reset the SLE4436
sle4436_verifyPassword(byte[]) - Method in class android.device.IccManager
  Submit the transfer data, enter the personalization mode
sle4436_writeBit() - Method in class android.device.IccManager
  Write a byte for Card
sle4436_writeCarry(int, int, byte[], int) - Method in class android.device.IccManager
  Write Carry data
sle4436_writeMemory(int, byte[], int) - Method in class android.device.IccManager
  Write data to the main storage area SLE4436
sle4442_changePassword(byte[]) - Method in class android.device.IccManager
  Change password.
sle4442_readErrorCounter(byte[]) - Method in class android.device.IccManager
  Change password.
sle4442_readMainMemory(int, int) - Method in class android.device.IccManager
  Read the data stored in main memory for SLE4442
sle4442_readProtectionMemory(int, int) - Method in class android.device.IccManager
  Read SLE4442 card protection bit storage data (4 BYTE). 4 bytes of data read is to save the SLE4442 bits data in storage area.
sle4442_reset(byte[]) - Method in class android.device.IccManager
  reset the SLE4442
sle4442_verifyPassword(byte[]) - Method in class android.device.IccManager
  Comparison of SLE4442 cards, each card after power compared to the card password, otherwise the card data is read-only, you will not be on the card of any write operation.
sle4442_writeMainMemory(int, byte[], int) - Method in class android.device.IccManager
  Write data to the main storage area SLE4442
sle4442_writeProtectionMemory(int, byte[], int) - Method in class android.device.IccManager
  The write protection bit storage area.
startDecode() - Method in class android.device.ScanManager
  Call this method to start decoding.
stopDecode() - Method in class android.device.ScanManager
  This stops any data acquisition currently in progress.
switchOutputMode(int) - Method in class android.device.ScanManager
  Use this function to set the output mode of the barcode reader (either send output to text box or as Android intent).
Symbology - Enum in android.device.scanner.configuration
  `Symbology` is an enumeration class defining constants for different barcode types.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W