Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## T

TIMEOUT_BETWEEN_SAME_SYMBOL - Static variable in class android.device.scanner.configuration.PropertyID
  To set Scanner decoding timeout between same symbol Parameters Values: value * 100 ms VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_min 1 VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_max 99 VALUE_TIMEOUT_BETWEEN_SAME_SYMBOL_Default 10
toInt() - Method in enum android.device.scanner.configuration.Symbology
  Converts the Symbology to its corresponding integer value.
toInt() - Method in enum android.device.scanner.configuration.Triggering
Triggering - Enum in android.device.scanner.configuration
  Trigger decode Mode

  CONTINUOUS A trigger pull activates the laser and decode processing.

TRIGGERING_LOCK - Static variable in class android.device.scanner.configuration.PropertyID
TRIGGERING_MODES - Static variable in class android.device.scanner.configuration.PropertyID
  To set Scanner trigger modes Parameters Values: `Triggering`
TRIOPTIC - Static variable in class android.device.scanner.configuration.Constants.Symbology
TRIOPTIC_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
type - Variable in class android.device.KeyMapManager.KeyEntry
  Describes `KeyMapManager.KEY_TYPE_KEYCODE` or `KeyMapManager.KEY_TYPE_STARTAC`

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W