Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## M

m1_amount(int) - Method in class android.device.PiccManager
  read the amount for the block number
m1_decrement(int, int) - Method in class android.device.PiccManager
  decrement the value block by iMoney amount
m1_increment(int, int) - Method in class android.device.PiccManager
  increment the value block by iMoney amount
m1_init(int, int) - Method in class android.device.PiccManager
  init the value block by value
m1_keyAuth(int, int, int, byte[], int, byte[]) - Method in class android.device.PiccManager
  authenticate a key
m1_readBlock(int, byte[]) - Method in class android.device.PiccManager
  To read a block
m1_restore(int) - Method in class android.device.PiccManager
  Move the content of a block into temporary data register
m1_transfer(int) - Method in class android.device.PiccManager
  transfer from temporary internal data register to value block
m1_writeBlock(int, int, byte[]) - Method in class android.device.PiccManager
  Write a block into the card
M25_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
MagManager - Class in android.device
  The MagManager class is used to initialize and control the MSR card reader.
MagManager() - Constructor for class android.device.MagManager
mapKeyEntry(KeyEvent, int, String) - Method in class android.device.KeyMapManager
  Create a new key event remap that is the same as the given one, but whose keycode is replaced with the given value.
MATRIX25 - Static variable in class android.device.scanner.configuration.Constants.Symbology
MAXICODE - Static variable in class android.device.scanner.configuration.Constants.Symbology
MAXICODE_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
MICROPDF417 - Static variable in class android.device.scanner.configuration.Constants.Symbology
MICROPDF417_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
MICROQRCODE_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
MSI - Static variable in class android.device.scanner.configuration.Constants.Symbology
MSI_CHECK_2_MOD_11 - Static variable in class android.device.scanner.configuration.PropertyID
MSI_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
MSI_LENGTH1 - Static variable in class android.device.scanner.configuration.PropertyID
MSI_LENGTH2 - Static variable in class android.device.scanner.configuration.PropertyID
MSI_REQUIRE_2_CHECK - Static variable in class android.device.scanner.configuration.PropertyID
MSI_SEND_CHECK - Static variable in class android.device.scanner.configuration.PropertyID
MULTI_DECODE_MODE - Static variable in class android.device.scanner.configuration.PropertyID

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W