Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## R

request(byte[], byte[]) - Method in class android.device.PiccManager
  Request card
request_norats(byte[], byte[]) - Method in class android.device.PiccManager
  Request card and no enable RATS
request_Type(byte[]) - Method in class android.device.IccManager
  Request IC Card type.
request_type(byte, byte[], byte[]) - Method in class android.device.PiccManager
  Request Specify card type
RESERVED_13 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_15 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_16 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_20 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_21 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_27 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_28 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_30 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_33 - Static variable in class android.device.scanner.configuration.Constants.Symbology
RESERVED_6 - Static variable in class android.device.scanner.configuration.Constants.Symbology
resetScannerParameters() - Method in class android.device.ScanManager
  Set factory defaults for all barcode symbology types.
ROYAL_MAIL_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
ROYAL_MAIL_SEND_CHECK - Static variable in class android.device.scanner.configuration.PropertyID

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W