Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## G

generateRandomData(byte[], byte[]) - Method in class android.device.SEManager
  Generate a 8 bytes random number.
getAllStripInfo(byte[]) - Method in class android.device.MagManager
  Get information on all 3 strips
getDeviceId() - Method in class android.device.DeviceManager
  Get the device product serial number
getDockerState() - Method in class android.device.DeviceManager
  Support i9000S(Android 4.3/Android5.1) only.Return the currently active docking station connected state .
getEncryptStripInfo(int, int, byte[], byte[], byte[]) - Method in class android.device.MagManager
  Get information on all 3 Encrypt strips data and plain text card NO.
getFirmwareVersion(byte[], byte[]) - Method in class android.device.SEManager
  get security processor firmware version.
getKeyAction(int) - Method in class android.device.KeyMapManager
  Returns special actions if this scan code is a KeyEvent keycode.
getKeyCode(int) - Method in class android.device.KeyMapManager
  Returns new keycode if this scan code is a KeyEvent keycode.
getKeyList() - Method in class android.device.KeyMapManager
  Returns all remap keys describes.
getKeyMeta(int) - Method in class android.device.KeyMapManager
getKeytype(int) - Method in class android.device.KeyMapManager
  Returns ramap type if this scan code is a KeyEvent keycode.
getOutputMode() - Method in class android.device.ScanManager
  get current the scan result output mode
getParameterInts(int[]) - Method in class android.device.ScanManager
  Gets one or more programming parameters of type Integer from the scan engine
getParameterString(int[]) - Method in class android.device.ScanManager
  Gets label programming parameters of type String at the specified indexs.
getPinBlock(int, int, byte[], int, String, long, SEManager.PedInputListener) - Method in class android.device.SEManager
  Get the pin block.
getPinBlockEx(int, int, byte[], int, String, long, String, SEManager.PedInputListener) - Method in class android.device.SEManager
  Get the pin block.
getPinBlockEx(android.os.Bundle, SEManager.PedInputListener) - Method in class android.device.SEManager
  Get the pin block.
getResponseEnable(byte) - Method in class android.device.IccManager
  Set whether the drive layer to the 61xx, 6Cxx and other commands for automatic data acquisition, the default for automatic acquisition.
getScannerState() - Method in class android.device.ScanManager
  get the scanner power states
getSingleStripInfo(int, byte[]) - Method in class android.device.MagManager
  Get specific strip information
getStatus() - Method in class android.device.PrinterManager
  Gets the current state of the printer `PrinterManager.PRNSTS_OK` `PrinterManager.PRNSTS_OUT_OF_PAPER` `PrinterManager.PRNSTS_OVER_HEAT` `PrinterManager.PRNSTS_UNDER_VOLTAGE` `PrinterManager.PRNSTS_BUSY` `PrinterManager.PRNSTS_ERR` `PrinterManager.PRNSTS_ERR_DRIVER` Returns the printer status. 0 for status OK
getStatus(byte[], byte[]) - Method in class android.device.SEManager
  get security processor hardware status
getTIDSN() - Method in class android.device.DeviceManager
getTriggerLockState() - Method in class android.device.ScanManager
  get the scan trigger status
getTriggerMode() - Method in class android.device.ScanManager
  Returns current configure triggering decode mode.
GOOD_READ_BEEP_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
GOOD_READ_VIBRATE_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
GS1_128 - Static variable in class android.device.scanner.configuration.Constants.Symbology
GS1_14 - Static variable in class android.device.scanner.configuration.Constants.Symbology
GS1_14_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
GS1_14_TO_UPC_EAN - Static variable in class android.device.scanner.configuration.PropertyID
GS1_EXP - Static variable in class android.device.scanner.configuration.Constants.Symbology
GS1_EXP_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
GS1_EXP_LENGTH1 - Static variable in class android.device.scanner.configuration.PropertyID
GS1_EXP_LENGTH2 - Static variable in class android.device.scanner.configuration.PropertyID
GS1_LIMIT - Static variable in class android.device.scanner.configuration.Constants.Symbology
GS1_LIMIT_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W