Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W

## A

action - Variable in class android.device.KeyMapManager.KeyEntry
  Describes the special actions to start APPS`android.content.Intent`
ACTION_DECODE - Static variable in class android.device.ScanManager
activate(byte[]) - Method in class android.device.IccManager
  Activate and reset the card
activate() - Method in class android.device.PiccManager
  activate card to start sending APDU。
activateEx(byte[]) - Method in class android.device.PiccManager
  activate card to start sending APDU。
android.device - package android.device
android.device.scanner.configuration - package android.device.scanner.configuration
antisel(byte[], byte[]) - Method in class android.device.PiccManager
  anti-collision and select card and returns the serial number of the card
apduTransmit(byte[], int, byte[], byte[]) - Method in class android.device.IccManager
  Transmit APDU to the IC card
apduTransmit(byte[], int, byte[], byte[]) - Method in class android.device.PiccManager
  Transmit APDU commands
apduTransmit(byte[], int, byte[]) - Method in class android.device.PiccManager
  Transmit APDU exchange commands:e.g.
apduTransmit(byte[], int, byte[], int, int) - Method in class android.device.PiccManager
  Transmit APDU exchange commands:e.g.
apduTransmit(int, int, byte[], int, byte[]) - Method in class android.device.PiccManager
  Transmit APDU commands for F Card
at88sc102_read(int, int) - Method in class android.device.IccManager
  Read the data stored in main memory for At88sc102
at88sc102_VerifyPassword(int, byte[], int) - Method in class android.device.IccManager
  Check & Verify password for At88sc102.
at88sc102_write(int, byte[], int) - Method in class android.device.IccManager
  Write data to the main storage area At88sc102
AUSTRALIAN_POST_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
AZTEC - Static variable in class android.device.scanner.configuration.Constants.Symbology
AZTEC_ENABLE - Static variable in class android.device.scanner.configuration.PropertyID
AZTEC_INVERSE - Static variable in class android.device.scanner.configuration.PropertyID

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV LETTER NEXT LETTER | FRAMES NO FRAMES

A B C D E F G H I J K L M N O P Q R S T U V W